No Till Drill Check List

Inspect the following

Frame- cracks, dents, and other damage

Wheels- pressure and condition

Chains- make sure they are in operable condition

Hydraulic hoses- Condition

Wiring harness- operational

All drives- do they turn freely

Machine lubrication- all parts properly greased

Feeder cups- blown out and free from obstruction

Guards- Are they there and working

If you have questions call 906 753 6921 ext. 101 or 906 753 2322